DN-300C Firmware Update Instructions

* Put the firmware file in the Root Directory of a USB drive; be sure to unzip the file so the file labeled [*1FX7P19018\_DP13\_64M.fwu*](http://redmine.inmusicbrands.com/attachments/download/35087/1FX7P19018_DP13_64M.fwu) appears in the root of the drive.
* Power on the DN-300C.
* Press the source button to enter USB mode.
* Insert the USB drive with firmware into USB port on the front panel.
* Instantaneously there will be a prompt asking the user to update the firmware, press the play/pause button on the front panel within the 5 second countdown.
  + If you do not press the play/pause button then the DN-300C will bypass the firmware update.
  + If you miss the countdown but still want to update the firmware remove the USB drive from the port and start this process again.
* You will see the update status on the screen, after the update is complete the DN-300C will reset and normal operation will occur.